Open topic with navigation

# [afp] Module Configuration

The `afp` module identifies indexed audio sections.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `fp` | `tr` | Receives AFP feature data, and identifies indexed audio sections.

Example:

    tr <- afp (_, fp)

## Parameters

Delay |
FpDb* |
MinDuration |
MinHits |
MinRate |
NBest |
SampleFrequency |
TimeQuant |

*You must set the value of this configuration parameter by setting the corresponding action parameter.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm