Open topic with navigation

# [sidpackager] Module Configuration

The `sidpackager` module creates an .ast speaker identification package from a set of individual speaker models. This module also calculates the speaker match thresholds based on statistics generated during the optimization stage.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
`BALANCED` |  |  | Calculates speaker thresholds based on balancing false negatives with false positives.
`MAXFAR` |  |  | Calculates speaker thresholds based on restricting the false positive rate to a specified threshold.

Examples:

    output <- sidpackager(BALANCED, input)

    output <- sidpackager(MAXFAR, input)

## Parameters

AstFileOut* | SpkIDBasePack
AstFileOutLabel* | SpkListFile*
BalanceBias | SpkListPath
BaseAstFile* | SpoFile*
Diag | SpoListFile*
DiagFile | SpoListPath*
DiagFileLabel | USMEnabled *
MaxFar | USMFile *
MaxFarFile |

*You must set the value of these configuration parameters by setting the corresponding action parameters.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm