Open topic with navigation

# MinPhoneRate

The minimum phone rate (phones per second) that a segment must have in order to be considered valid.

Type: | String
Default: | 1.0
Range: | 0.0 - 2.0
Required: | No
Configuration Section: | langid module
Example: | `MinPhoneRate=1.0`
See Also: | MinPhoneRate (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm