Open topic with navigation

# MLLRMaxMins

Whether to use standard acoustic adaptation or rapid adaptation mode. The default value (`0`) specifies standard acoustic adaptation mode. Where less adaptation data is available, setting a value of `10000000` enables rapid adaptation mode. Use the rapid adaptation mode in conjunction with a single accumulator file. The standard mode can combine multiple accumulator files.

Note: Currently, you can specify only the values `0` or `10000000`. The use of fixed values rather than a simple Boolean allows the possibility of a future extension to automatically decide whether to use rapid or full adaptation modes.

Type: | Integer
Default: | 0 (rapid adaptation mode is disabled)
Range | 0 or 10000000
Required: | No
Configuration Section: | amadaptadddata module
Example: | `MLLRMaxMins=10000000`
See Also: | MLLRMaxMins (action parameter) MLLRMinOcc Relevance

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm