Open topic with navigation

# SpkIdTrain

The `SpkIdTrain` task uses the set of feature files that you created by using the SpkIdFeature task to train a new speaker template.

If you are using multiple feature files, you must create a list file that contains a list of all the feature files. You can do this manually, or by using the List Manager.

Each element of the list should be the file name relative to the Speaker ID directory, and must include the file extension. For example:

    BrownSpeech1.atv
    BrownSpeech2.atv
    BrownSpeech3.atv

Note: If the files are not stored in the Speaker ID directory, you can use the DataPath parameter to specify the location.

For more information about HPE IDOL Speech Server's list manager, see the HPE IDOL Speech Server Administration Guide.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Set to `SpkIdTrain`. | Yes
DataExt | The file extension to use alongside the list entry, if not specified in the entry. |
DataFile | A single input feature file to use to train the template. | Yes, if `DataList` is not set
DataList | A list file that lists the feature files to use. | Yes, if `DataFile` is not set.
DataPath | The path to the directory containing the feature files. |
DiagFile | The name of the file to write diagnostic information to. |
DiagLevel | The level of detail to include in the diagnostic information. |
LabExt | The file extension to use for label files. | Yes, if your files have an extension other than the default (`.lab`)
LabFile | A single label file to use. |
LabPath | The path to the label files. | Yes, if you have enabled labeling and are specifying a list of multiple files to use
LabType | The type of labels to use. |
Out | The name of the speaker template file to create. You must include the audio template file extension (`.atf`). | Yes
Sfreq | The sample frequency of the audio file to process. |
UBMFile | The Universal Background Model to use. |

## Example

`http://localhost:15000/action=AddTask&Type=SpkIdTrain&DataList=ListManager/BrownList&Out=Brown.atf`

This action uses port `15000` to instruct HPE IDOL Speech Server, which is located on the local machine, to create the `Brown.atf` template using the feature files listed in the `BrownList` list file.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm