Open topic with navigation

# SpeechSilClassification

The `SpeechSilClassification` task segments an audio file by content, classifying each segment as either speech, non-speech, or music.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Set to `SpeechSilClassification`. | Yes
AppDnnBase | The location of the `appResources` directory, which contains the DNN and `.ian` files to use. |
EndTime | The end of an audio section to process. |
File | The audio file to process. | Yes
FrameDupl | The balance between performance and speed for audio preprocessing DNN classification. |
MaxSegSize | The maximum audio class size in frames. |
MinSegSize | The minimum segment size in frames. |
Out | The file to write the results to. | Yes
Sfreq | The sample frequency of the audio file to process. |
SilThresh | The threshold between what the task identifies as silence and non-silence. |
SpeechThresh | The threshold between speech and non-speech (music or noise). |
StartTime | The beginning of an audio section to process. |
SugdInputChannels | The channel layout of the input media file. |
SugdInputFrequency | The sampling rate of the input media file. |

## Example

    http://localhost:13000/action=AddTask&Type=SpeechSilClassification&File=C:\Data\Conference.wav&Out=ConfClassification.ctm

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to segment and classify the `Conference.wav` file and to write the results to the `ConfClassification.ctm` file.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm