Open topic with navigation

# [amadaptend] Module Configuration

The `amadaptend` module reads in a set of accumulator files produced during adaptation data ingestion, and writes an updated acoustic model file.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
|  |  | The `amadaptadddata` module does not accept input streams or write to an output stream. All inputs and outputs are file based.

Example:

    output ← amadaptadddata(–, input)

## Parameters

AccExt | MinEgs
AccListFile* | OutAmFile*
AccPath | Relevance
InAmFile* | UpdateWeights

*You must set the value of these configuration parameters by setting the corresponding action parameters.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm