Open topic with navigation

# MaxFar

The `MaxFar` parameter sets the maximum permissible False Acceptance Rate (FAR). The False Acceptance Rate is the expected rate at which segments are labeled incorrectly as coming from a particular speaker.

The `MaxFar` rate is estimated from the provided development data. In general, reducing `MaxFar` increases the False Rejection Rate (FRR)—the rate at which segments from a particular speaker are labeled incorrectly.

Action: | AddTask, CheckResources
Task: | SidPackage
Type: | Decimal
Default: | 0.1
Range: | 0.01–0.99
Example: | `MaxFar=0.5`
See Also: | MaxFar (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm