Open topic with navigation

# MinFrames

The minimum number of speech audio frames required to train each component of a speaker model.

During training, HPE IDOL Speech Server creates several components (mixtures), up to a maximum specified in the NMix parameter. Each component must be trained on a minimum amount of data, specified in the `MinFrames` parameter. If there is not enough data available, HPE IDOL Speech Server trains fewer components and the speech model performs less well.

Action: | AddTask, CheckResources
Task: | StreamSidTrain, WavSidTrain
Type: | Integer
Default: | 500
Range: | 50–5000
Example: | `MinFrames=4000`
See Also: | MinFrames (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm