Open topic with navigation

# OutAm

The file to write the adapted acoustic model to.

You can specify an absolute or relative file path. If you specify a relative path, it is considered as being relative to the acoustic model directory. If the file path is excluded, HPE IDOL Speech Server defaults to the acoustic model directory.

Note: The TrainedAmDir parameter in the `[Paths]` section of the configuration file sets the location of the acoustic model directory.

Action: | AddTask, CheckResources
Task: | AmTrainFinal
Type: | String
Default: |
Example: | `OutAm=myModel.am`
See Also: | OutAmFile (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm