Open topic with navigation

# SampleFrequency

The `SampleFrequency` parameter specifies the sampling frequency of the audio (the frames produced by the module).

Note: If the FFmpeg library is enabled, the `wav` module can accept a variety of audio formats with different sampling frequencies. In such cases, the `wav` module converts the audio to the specified sampling frequency.

Note: To detect breaking glass using the `audiosec` module, HPE strongly recommends that the audio sampling rate is 16000 Hz.

Type: | Integer
Default: | 16000 (No default value for the `sidfeature`, `sidoptimizer`, and `speakerid` modules.
Range: | 8000 or 16000
Required: | Only for the `sidfeature`, `sidoptimizer`, and `speakerid` modules
Configuration Section: | afp, afpfeature, audiopreproc, audiosec, audiotemplatedevel, audiotemplatescore, audiotemplatetrain, frontend, normalizer, sidfeature, sidoptimizer, sidpackager, sidtrain, speakerid, splitspeech, stream, and wav modules
Example: | `SampleFrequency=16000`
See Also: | Sfreq (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm