Open topic with navigation

# DiagLevel

The level of detail to include in the diagnostic information.

Set `DiagLevel` to a value between `0` and `3`. The higher the setting, the more information is included in the diagnostic file.

Action: | AddTask
Task: | SpkIdDevel , SpkIdDevelFinal , SpkIdDevelStream , SpkIdEvalStream ,SpkIdTrain, SpkIdTrainStream, SpkIdTrainWav
Type: | Integer
Default: |
Example: | `DiagLevel=3`
See Also: | DiagLevel (configuration parameter) DiagFile

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm