Open topic with navigation

# DTMF Identification

The `audiopreproc` module can perform DTMF (Dual-Tone Multi-Frequency) dial tone detection and identification. In this mode, the module can accurately detect and identify tones corresponding to the numbers 0-9, the letters A-D, and the asterisk (*) and hash (#) keys.

To enable DTMF dial tone identification, set the `audiopreproc` mode to `T`. For an example schema incorporating DTMF dial tone identification, see Identify DTMF Dial Tones. This schema produces a stream of DTMF labels (such as `<DTMF-1>`, `<DTMF-A>` or `<DTMF-#>`).

© 2013-2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm