Open topic with navigation

# [amadaptadddata] Module Configuration

The `amadaptadddata` module accepts acoustic adaptation audio and transcript data, along with an existing acoustic model, and analyzes the data and how well the current model fits with the data. It creates an accumulator file that is subsequently used to update the acoustic model parameters.

Note: Currently you can adapt only GMM models, not the newer, better-performing DNN acoustic models. Generally, GMM model adaptation produces models that are still inferior to the out-of-the-box performance of DNN models.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
|  |  | The `amadaptadddata` module does not accept input streams or write to an output stream. All inputs and outputs are file based.

Example:

    output <- amadaptadddata(–, input)

## Parameters

AccFile* | JunkEnabled | PlhExt
AdaptSil | JunkWordThreshold | PlhPath
AddOptSil | MaxBeamValue | SilConstrain
AmFile* | MinBeamValue | TimeConstrain
BeamStep | MLLRMaxMins | TimeRelax
DataListFile* | MLLRMinOcc | TxtExt
DctFile | OutLabExt | TxtPath
Diag | OutLabPath | WriteOutLabs
DiagFile | PgfFile | ZeroDurationWords

*You must set the value of these configuration parameters by setting the corresponding action parameters.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm