Open topic with navigation

# Gb_MinStreaks

The `Gb_MinStreaks` parameter specifies the minimum number of distinct frequency streaks.

Type: | Integer
Default: | 10
Recommended Range: | Minimum: 8 Maximum: 16
Required: | No
Configuration Section: | audiosec module
Example: | `Gb_MinStreaks=10`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm