Open topic with navigation

# Sfreq

The sample frequency of the audio file to process–either `8000` or `16000`. If not set, HPE IDOL Speech Server assumes a default of `16000`.

Action: | AddTask, CheckResources
Task: | AfpAddTrackStream, AfpAddTrackWav, AfpMatchStream, AfpMatchWav, AfptAddTrackStream , AfptAddTrackWav , AfptMatchWav, ClippingDetection, DialToneIdentification, SidTrain, SidTrainFinal, SNRCalculation, SpeechSilClassification, SpkIdDevel , SpkIdDevelStream , SpkIdDevelFinal , SpkIdDevelWav, SpkIdEvalStream , SpkIdFeature , SpkIdTrain, SpkIdTrainStream, SpkIdTrainWav, StreamSidOptimize, StreamSidTrain, StreamSpeakerId, WavSidOptimize, WavSidTrain, WavToPlh
Type: | Integer
Default: | 16000
Example: | `Sfreq=8000`
See Also: | SampleFrequency (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm