Open topic with navigation

# MaxSegSize

The maximum segment size in frames (a frame is 10 ms duration). This value must be more than three times the specified MinSegSize.

Note: Setting `MaxSegSize` to a lower value leads to less accuracy. Setting `MaxSegSize` to a high value leads to less resolution.

Type: | Integer
Default: | 300
Recommended Range: | Minimum: 50 Maximum: 3000
Required: | No
Configuration Section: | audiopreproc module
Example: | `MaxSegSize=150`
See Also: | MaxSegSize (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm