Open topic with navigation

# AudioAnalysis

The `AudioAnalysis` task runs all the audio preprocessing tasks that are supported by the `audiopreproc` module in a single task.

For more information, see [audiopreproc] Module Configuration.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Specify `AudioAnalysis`. | Yes
AppDnnBase | The location of the `appResources` directory, which contains the DNN and `.ian` files to use. |
CtmFile | The speech-to-text transcript produced for the audio file. | Yes
File | The audio file to process. | Yes
FrameDupl | The balance between performance and speed for audio preprocessing DNN classification. |
Out | The XML file to write the audio analysis results to. | Yes
Sfreq | The sample frequency of the audio file to process. |
SugdInputChannels | The channel layout of the input media file. |
SugdInputFrequency | The sampling rate of the input media file. |

## Example

    http://localhost:13000/action=AddTask&Type=AudioAnalysis&File=C:\data\Sample.wav&Out=SampleAnalysis.xml

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to perform audio analysis on the `Sample.wav` file and to write the results to the `SampleAnalysis.xml` file.

The `AudioAnalysis` log file provides information on several audio quality assessments. For example:

    <autnresponse>
        <audiopreproc>
            <snr>
                <mean>20</mean>
                <audio_level>66</audio_level>
            </snr>
            <gain>
                <size>35</size>
                <energy>69</energy>
            </gain>
            <max_gain_difference>0</max_gain_difference>
            <clipping>
                <assessment>no</assessment>
                <percent_frames>0</percent_frames>
            </clipping>
            <categories>
                <speech_percent>77.3667</speech_percent>
                <silence_percent>7.45</silence_percent>
                <noise_music_percent>15.9</noise_music_percent>
            </categories>
        </audiopreproc>
        <resultDeleted>False</resultDeleted>
    </autnresponse>

The log file includes information on the following:

- The signal-to-noise ratio (SNR) of the file, including the mean SNR across the whole file, and an assessment of the audio level of any regions that contain speech.

- The gain level, and the actual energy level. The log file also includes a summary of the maximum difference in decibels between speaker levels across the whole file (`<max_gain_difference>`). For a good quality waveform where the two speakers speak at a similar gain level, this number can be zero (or at least very low).

- An assessment of the amount of clipping in the file, and the number of frames affected. The `<assessment>` field can hold one of the following values:

  `no` | no clipping
  `insignificant` | <= 0.1% of frames
  `minor` | <= 1% of frames
  `moderate` | <= 4% of frames
  `heavy` | > 4% of frames

- An estimate of the percentage of the file that is speech, silence, or noise or music.

You can use the `GetResults` action to retrieve this information; you do not need to specify a result label.

The `AudioAnalysis` task also produces an additional audio classification `.ctm` file. By default, this has the same name as the task token. You can use the `GetResults` action with the `label` parameter set to `class` to retrieve this file.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm