Open topic with navigation

# Run the Task

HPE IDOL Speech Server provides four preconfigured speech-to-text tasks:

- `WavToText`, which performs speech-to-text on an audio file
- `StreamToText`, which performs speech-to-text on an audio stream
- `StreamToTextMusicFilter`, which performs speech-to-text on an audio stream and categorizes the audio so that you can remove any sections categorized as music or noise from the resulting `.CTM` file.
- `TelWavToText`, which performs speech-to-text on audio files of telephone conversations. The task also detects and reports dial tones and DTMF dial tones (see DTMF Identification).

There are also four preconfigured speech-to-text tasks that perform speech-to-text but also include simple sentence-forming punctuation (for example, full stops and initial capital letters) in the `.CTM` file:

- `WavToTextPunct`
- `StreamToTextPunct`
- `StreamToTextMusicFilterPunct`
- `TelWavToTextPunct`

These tasks work in exactly the same way as their non-punctuated counterparts.You can also use the `PunctuateCtm` task has been added to add punctuation to any `.CTM` file. For more information, see the HPE IDOL Speech Server Reference.

To run speech-to-text on an audio file

- Send an `AddTask` action to HPE IDOL Speech Server, and set the following parameters:

  `Type` | The task name. Specify `WavToText`.
  `File` | The audio file to process. To restrict processing to a section of the audio file, set the start and end times in the `wav` module. For information about how to configure the `wav` module, see the HPE IDOL Speech Server Reference.
  `Out` | The file to write the transcription to.
  `Lang` | The language pack to use.

For example:

    http://localhost:13000/action=AddTask&Type=WavToText&File=C:/myData/Speech.wav&Out=SpeechTranscript.ctm&Lang=ENUS

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to perform the `WavToText` task on the `Speech.wav` file and write the results to the `SpeechTranscript.ctm` file. The `Speech.wav` file contains U.S. English dialect speech.

If you are using a lattice file and want to reduce the lattice output size by including only one sample of each word in a specific window size, you can also set the `LatWinSize` parameter. See Use a Lattice File and the HPE IDOL Speech Server Reference for more information.

This action returns a token. You can use the token to:

- Check the task status. See Check the Status of a Task.
- Retrieve the results. The speech-to-text operation produces results while it crunches through the audio data, so you can retrieve results before the task is complete. See Find Recommended Language Resources to Use in a Task.

When you use HPE IDOL Speech Server to process multiple data streams or files at the same time, the server might not have enough CPU or memory to process all of them at once. Speech-to-text operation is very CPU-intensive. To check whether a server has sufficient resources to run a `WavToText` task, send a `CheckResources` action. See Check Available Resources.

© 2013-2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm