Open topic with navigation

# SegmentWindow

The `SegmentWindow` parameter sets the amount of audio considered at any point when detecting the boundaries where the detected language changes. The units are in frames (a frame is 10 ms).

Increasing this number can lead to more reliable boundary detection, however the exact boundary time reported might be less precise.

Type: | Integer
Default: | 150
Range: | 100–500
Required: | No
Configuration Section: | langid module (`BOUNDARY` mode only)
Example: | `SegmentWindow=150`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm