Open topic with navigation

# LangIdBndWav

The `LangIdBndWav` task reads in data from an audio file, converts it into language identification features, and determines boundaries where the language changes. The task returns the language identification results between boundaries.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Set to `LangIdBndWav`. | Yes
AppDnnBase | The location of the `appResources` directory, which contains the DNN and `.ian` files to use. |
Beam | The beam width of the search process. |
ClassList | A list of language classifiers to use. |
ClassPath | The path to the directory containing the language classifiers. |
DnnFile | The Deep Neural Network acoustic modeling file to use. |
File | The audio file to process. | Yes
FrameDupl | The balance between performance and speed for audio preprocessing DNN classification. |
Lang | The name of the language pack to use. | Yes
LangList | A subset of languages to use from the classifier list file. |
MinPhoneRate | The minimum phone rate (phones per second). |
NBest | The maximum number of language candidates to include in the output file. |
Out | The file to write language identification results to. | Yes
OutB | The file to write boundary point information to. | Yes
SegSize | The maximum results segment size. |
SegSmoothWin | The size of the smoothing window. |
SegStep | The step size in phones of the analysis window. |
SilThresh | The threshold between what the task identifies as silence and non-silence. |
SpeechThresh | The threshold between speech and non-speech (music or noise). |
SugdInputChannels | The channel layout of the input media file. |
SugdInputFrequency | The sampling rate of the input media file. |

Note: The `ClassList` parameter is required only if you want to change the audio sample rate, or if you want to use your own custom classifiers. You might also need to specify the `ClassPath` parameter, depending on the location of the classifier files.

## Example

    http://localhost:13000/action=AddTask&Type=LangIdBndWav&File=C:\Data\Speech.wav&ClassList=ListManager/OptClassSet&ClassPath=C:\LangID\&Out=SpeechLang1.ctm&OutB=SpeechBnd.ctm

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to identify languages and language boundaries in the `Speech.wav` file using the language classifiers specified in the `OptClassSet` list. The action instructs HPE IDOL Speech Server to write the identification results to the `SpeechLang1.ctm` file and the boundary information to the `SpeechBnd.ctm` file.

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm