Open topic with navigation

# MaxSeg

The maximum duration of an audio segment in seconds, when segmenting audio based on speaker or class identification.

Action: | AddTask, CheckResources
Task: | SegmentWav
Type: | Decimal
Default: | 32.0
Range: | 5–60
Example: | `MaxSeg=50`
See Also: | SegMax (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm