Open topic with navigation

# SugdInputFrequency

Specifies the sampling rate of the input media file. This parameter applies only if the FFmpeg library is enabled, allowing conversion of audio files. HPE IDOL Speech Server first attempts to determine the sampling rate from the file that it receives. If it is unsuccessful, HPE IDOL Speech Server uses the value specified by the `SugdInputFrequency` parameter.

Type: | Integer
Default: | None
Required: | No
Configuration Section: | wav, sidtrain, and splitspeech modules
Example: | `SugdInputFrequency=44100`
See Also: | SugdInputFrequency (action parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm