Open topic with navigation

# Al_TmThreshold

The `Al_TmThreshold` parameter specifies the template match (cross correlation) threshold for alarm identification.

Type: | Decimal
Default: | 0.3
Range: | 0.2–0.5
Required: | No
Configuration Section: | audiosec module
Example: | `Al_TmThreshold=0.3`
See Also: |

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm