Open topic with navigation

# [afpfeature] Module Configuration

The `afpfeature` module converts raw audio data into AFP feature data that HPE IDOL Speech Server can use to identify sections of audio using the `afp` module.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `a` | `fp` | Receives raw audio data and converts it into AFP feature data.

Example:

    fp <- afpfeature(_, a)

## Parameters

Alts

RndSample

SampleFrequency

SpecSize

Sqecquant

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm