Open topic with navigation

# [amadaptend] Module Configuration

The `amadaptend` module reads in a set of accumulator files produced during adaptation data ingestion, and writes an updated acoustic model file.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
|  |  | The `amadaptadddata` module does not accept input streams or write to an output stream. All inputs and outputs are file based.

Example:

    output ← amadaptadddata(–, input)

## Parameters

AccExt

AccListFile

AccPath

InAmFile

MinEgs

OutAmFile

Relevance

UpdateWeights

Some of these parameters do not have an internal default value. You must either set the configuration parameter to a suitable value, or set the value in the corresponding action parameter.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm