Open topic with navigation

# Configure Audio Preprocessing Tasks

When you configure a task that uses the `audiopreproc` module, you must use the appropriate mode for the task that you want to perform. The following modes are available:

`A` | Audio categorization.
`C` | Clipping detection and assessment.
`S` | Signal-to-noise ratio calculation.
`T` | DTMF dial tone identification.

You can use one or more of these modes in a single schema. To use multiple modes, type the letter for each mode in the schema, without spaces. For example:

    1 = w1,d <- audiopreproc(CATS,a)

This example uses all four of the `audiopreproc` module modes to analyze audio.

For examples and more information on how to configure tasks, see Sample Task Schemas.

Related Topics

- Categorize Audio
- Assess Audio Quality
- Identify DTMF Dial Tones

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm