Open topic with navigation

# MaxSegSize

The maximum segment size in frames (a frame is 10 ms duration). This value must be more than three times the specified MinSegSize.

NOTE:

Setting `MaxSegSize` to a lower value leads to less accuracy. Setting `MaxSegSize` to a high value leads to less resolution.

Action: | AddTask CheckResources
Task: | SpeechSilClassification
Type: | Integer
Default: | 300
Range: | 50–3000
Example: | `MaxSegSize=50`
See Also: | MaxSegSize (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm