Open topic with navigation

# MinRate

The minimum hit rate threshold for audio fingerprint identification. Each hit is the identification of a single audio fingerprint feature (an audio fingerprint consists of a sequence of features).The `MinRate` value is the number of hits for each frame (one frame is 10 ms) that a section must generate before HPE IDOL Speech Server returns it as a match for a clip in an audio fingerprinting database.

Action: | AddTask CheckResources
Task: | AfpMatchStream AfpMatchWav AfptMatchStream AfptMatchWav
Type: | Float
Default: | 0.001
Range: | 0.001–0.01
Example: | `MinRate=0.006`
See Also: | MinRate (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm