Open topic with navigation

# Two Pass Alignment

HPE recommends two-pass alignment if the alignment quality is poor or if large sections of audio have not been aligned. This situation can arise when aligning very long audio. In two-pass alignments, alignment occurs over two steps:

1. Use `TranscriptCheck` to produce approximate timings for the transcript.

2. Perform alignment at the `prons` level by using the T`ranscriptCheck` approximate transcript time output file.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm