Open topic with navigation

# [wav] Module Configuration

The `wav` module reads mono or stereo media data from file, and can pass the data to other modules for further processing.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
`MONO` |  | `a` | Reads a mono media file.
`STEREO` |  | `l`, `r` | Reads a stereo media file.
`MONO_WRITE` | `a` |  | Writes a mono media file.
`MONO_DATA` |  | `a` | Reads in mono audio as a binary data block.
`STEREO_DATA` |  | `l`, `r` | Reads in stereo audio as a binary data block.

Examples:

    a <- wav(_, input)

    l, r <- wav(_, input)

## Parameters

EndTime

SampleFrequency

StartTime

SugdInputChannels

SugdInputFrequency

WavFile

Some of these parameters do not have an internal default value. You must either set the configuration parameter to a suitable value, or set the value in the corresponding action parameter.

NOTE:

If you do not set the WavFile parameter, but you have submitted some binary audio data (POST/Multipart), then the server uses the binary data block as the audio data source. If there is no task data available and you have not set the WavFile parameter, then the server returns an error.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm