Open topic with navigation

# SegMax

The `SegMax` parameter sets the maximum duration of an audio segment in seconds. It is used to segment audio based on the speaker or class identification.

Type: | Decimal
Default: | 32.0
Range: | 5–60
Required: | No
Configuration Section: | segment module
Example: | `SegMax=60`
See Also: | MaxSeg (action parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm