Open topic with navigation

# StreamToTextMusicFilterPunct

The `StreamToTextMusicFilterPunct` task takes a stream and returns a file containing a text version of the wav file. Sections of the audio that are determined to be music are filtered out and not included in the transcript.Simple sentence-forming punctuation (such as full stops and initial capital letters) is included in the `.ctm` output.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task type. Set to `StreamToTextMusicFilterPunct`. | Yes
AppDnnBase | The location of the `appResources` directory, which contains the DNN and `.ian` files to use. |
ClassWordFile | The path to a list of new words and weightings to add to the language model at load time. |
Conf | Whether to generate word confidence scores. |
CustomLm | The custom language model to use. |
Diag | Whether to generate diagnostic information. |
DiagFile | The alignment diagnostics file to generate. |
DnnFile | The DNN file to use. |
DnnScale | The DNN output acoustic score scaling factor. |
FrameDupl | An integer value which allows for greater time efficiency with only a minimal loss of recognition accuracy. |
FrameDupl | The balance between performance and speed for audio preprocessing DNN classification. |
Lang | The language pack to use. |
LatFile | The name of the lattice file that contains word hypotheses. |
LatScale | The depth of the lattice. |
LatWinSize | The size (in seconds) of the lattice output window. |
LatWordFile | A list of words to find. |
NonSentFinalWords | A list of words that are unlikely to end a sentence. |
Out | The file to write language identification results to. |
PronFile | A file to use to either replace or add alternative pronunciations of words at language load time. |
SilThresh | The threshold between what the task identifies as silence and non-silence. |
SpeechThresh | The threshold between speech and non-speech (music or noise). |

## Example

    http://localhost:13000/action=AddTask&Type=StreamToTextMusicFilterPunct&SpeechThresh=-30&Out=Transcript1.ctm

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to transcribe the audio stream (using the specified threshold values to determine sections that contain music), and to write the results to the `Transcript1.ctm` file, with any sections determined to be music filtered out, and punctuation included.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm