Open topic with navigation

# [stt] Module Configuration

The `stt` module converts normalized speech frontend frame data into a text transcription.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `nf` | `w` | Accepts normalized feature frames and performs speech-to-text. Produces a word label stream.

Example:

    w <- stt (_, nf)

## Parameters

Diag

DiagFile

DiagFileLabel

DnnScale

EnableConfidence

FrameDupl

Lang

LatFile

LatScale

LatWordFile

Mode

ModeValue

SpeechBiasLevel

Some of these parameters do not have an internal default value. You must either set the configuration parameter to a suitable value, or set the value in the corresponding action parameter.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm