Open topic with navigation

# FrameDupl

An integer value which allows for greater time efficiency without significant change in recognition accuracy.

For example, if you set `FrameDupl` to `1`, the speed of propagation increases by approximately 50%, if set to `2`, by 67%, and if set to `3`, by 75%. HPE recommends that you do not increase `FrameDupl` beyond `4`, to maximise time efficiency as opposed to recognition accuracy.

NOTE:

Propagation is the process of using a DNN to map audio feature frames to phonemes. Propagation time is typically 50% of the processing time.

Action: | AddTask
Task: | IvSpkIdDevelStream IvSpkIdDevelWav IvSpkIdEvalStream IvSpkIdEvalWav IvSpkIdFeature IvSpkIdTrainStream IvSpkIdTrainWav StreamToText StreamToTextMusicFilter StreamToTextMusicFilterPunct StreamToTextPunct TelWavToText TelWavToTextPunct WavPhraseSearch WavToFMD WavToText WavToTextPunct
Type: | Integer
Default: | 0
Example: | `FrameDupl=1`
See Also: | FrameDupl (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm