Open topic with navigation

# [audiosec] Module Configuration

The `audiosec` module detects security-related audio signals including alarms, screams, gunshots, and breaking glass.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
| `a, nf` | `w` | The `audiosec` module requires both raw audio data and normalized frontend feature frames.

Example:

    w <- audiosec(_, a,nf)

## Parameters

Al_AllowUnkAlarm

Al_GenThreshold

Al_MaxPeriod

Al_TemplateListFile

Al_TemplatePath

Al_TmThreshold

Gb_EdgeMaxDist

Gb_EdgeTrigger

Gb_MinDuration

Gb_MinOutScore

Gb_MinStreaks

Gs_EdgeTrigger

Model

SampleFrequency

Sc_MinScreamLen

Sc_MinScreamPitch

Sc_MinScreamSegScore

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm