Open topic with navigation

# DoDialTones

There are two types of dial tone:

- Dual-Tone Multi-Frequency dial tones, used in voice-activated menus.
- Standard dial tones used in regular telephone calls.

Set `DoDialTones` to `False` to identify only Dual-Tone Multi-Frequency dial tones. Set `DoDialTones` to `True` if you want to identify both types of dial tone.

Action: | AddTask
Task: | DialToneIdentification TelWavToText TelWavToTextPunct
Type: | Boolean
Default: | True
Example: | `DoDialTones=True`
See Also: |

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm