Open topic with navigation

# MinBeamValue

The minimum beam value at which to attempt the adaptation pass.

Type: | Integer
Default: | 1000
Range: | 500–5000
Required: | No
Configuration Section: | amadaptadddata module
Example: | `MinBeamValue=1500`
See Also: | MinBeam (action parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm