Open topic with navigation

# [amadaptadddata] Module Configuration

The `amadaptadddata` module accepts acoustic adaptation audio and transcript data, along with an existing acoustic model, and analyzes the data and how well the current model fits with the data. It creates an accumulator file that is subsequently used to update the acoustic model parameters.

NOTE:

Currently you can adapt only GMM models, not the newer, better-performing DNN acoustic models. Generally, GMM model adaptation produces models that are still inferior to the out-of-the-box performance of DNN models.

## Input and Output

Mode | Input | Output | Description
--- | --- | --- | ---
|  |  | The `amadaptadddata` module does not accept input streams or write to an output stream. All inputs and outputs are file based.

Example:

    output <- amadaptadddata(–, input)

## Parameters

AccFile

AdaptSil

AddOptSil

AmFile

AudioAnalysisDir

BeamStep

DataListFile

DctFile

Diag

DiagFile

DnnFile

JunkEnabled

JunkWordThreshold

MaxBeamValue

MaxOtdLen

MinBeamValue

MLLRMaxMins

MLLRMinOcc

OtdPath

OutLabExt

OutLabPath

PgfFile

PlhExt

PlhPath

RandOtd

SilConstrain

TimeConstrain

TimeRelax

TxtExt

TxtPath

WriteOutLabs

ZeroDurationWords

Some of these parameters do not have an internal default value. You must either set the configuration parameter to a suitable value, or set the value in the corresponding action parameter.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm