Open topic with navigation

# [afpfile] Module Configuration

The `afpfile` module both writes AFP features to file and reads audio fingerprinting files from file.

## Input and Output

The afpfile module has three modes of operation.

Mode | Input | Output | Description
--- | --- | --- | ---
`FINGERPRINT_READ` |  | `fp` | The name of the AFP feature file to read from.
`FINGERPRINT_WRITE` | `fp` |  | The name of the AFP feature file to write to.
`FINGERPRINT_WRITE` | `fp, w` |  | The AFP feature file in which to write AFP features filtered by the word labels received from the `w` stream.

Examples:

    fp <- afpfile(FINGERPRINT_READ, fp)

    output <- afpfile(FINGERPRINT_WRITE, fp)

    output <- afpfile(FINGERPRINT_WRITE, fp, w)

## Parameters

AFPFile

Alts

RndSample

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm