Open topic with navigation

# Sfreq

The sample frequency of the audio file to process–either `8000` or `16000`. If not set, HPE IDOL Speech Server assumes a default of `16000`.

Action: | AddTask CheckResources
Task: | AfpAddTrackStream AfpAddTrackWav AfpMatchStream AfpMatchWav AfptAddTrackStream AfptAddTrackWav AfptMatchWav ClippingDetection DialToneIdentification IvSpkIdDevel IvSpkIdDevelFinal IvSpkIdDevelStream IvSpkIdDevelWav IvSpkIdEvalStream IvSpkIdEvalWav IvSpkIdFeature IvSpkIdTrain IvSpkIdTrainStream IvSpkIdTrainWav SNRCalculation SpeechSilClassification SpkIdDevel SpkIdDevelStream SpkIdDevelFinal SpkIdDevelWav SpkIdEvalStream SpkIdFeature SpkIdTrain SpkIdTrainStream SpkIdTrainWav WavToPlh
Type: | Integer
Default: | 16000
Example: | `Sfreq=8000`
See Also: | SampleFrequency (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm