Open topic with navigation

# UBMFile

The Universal Background Model to use.

By default, the modules use the UBM that is included in the base speaker ID pack. Set `UBMFile` to `NONE` if you do not wish to use a background model.

Action: | AddTask
Task: | SpkIdTrain SpkIdTrainStream SpkIdTrainWav
Type: | String
Default: | None (the default is derived from the base speaker ID pack)
Example: | `UBMFile=baseModel.ubm`
See Also: | UBMFile (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm