Open topic with navigation

# TelWavToText

The `TelWavToText` task converts a telephony audio file into a text transcript. In addition to transcribing speech, the task recognizes and transcribes dial tones including DTMF.

## Parameters

Parameter | Description | Required
--- | --- | ---
Type | The task name. Specify `TelWavToText`. | Yes
ClassWordFile | The path to a list of new words and weightings to add to the language model at load time. |
Conf | Whether to generate word confidence scores. |
CustomLm | The custom language model to use. |
Diag | Whether to generate diagnostic information. |
DiagFile | The alignment diagnostics file to generate. |
DnnFile | The DNN file to use. |
DnnScale | The DNN output acoustic score scaling factor. |
DoDialTones | The type of dial tone to identify. |
EndTime | The end of an audio section to process. |
File | The audio file to process. | Yes
ForceRecompoundOff | Whether to prevent recompounding. |
ForceRecompoundOn | Whether to force recompounding. |
FrameDupl | An integer value which allows for greater time efficiency with only a minimal loss of recognition accuracy. |
Lang | The language pack to use. | Yes
LatFile | The name of the lattice file that contains word hypotheses. |
LatScale | The depth of the lattice. |
LatWinSize | The size (in seconds) of the lattice output window. |
LatWordFile | A list of words to find. |
Mode | The algorithm mode for the speech-to-text process. |
ModeValue | The value of the parameter associated with the speech-to-text algorithm mode. |
Out | The file to write the transcription to. | Yes
PronFile | A file to use to either replace or add alternative pronunciations of words at language load time. |
Punctuation | Whether to add punctuation to the word data. |
SilThresh | The threshold between what the module identifies as silence and non-silence. |
SpeedBiasLevel | The balance between speed and accuracy in the decoder. |
StartTime | The beginning of an audio section to process. |
SugdInputChannels | The channel layout of the input media file. |
SugdInputFrequency | The sampling rate of the input media file. |
WordBar | Switches on word barring. |
WordBarList | The location of a list of words to be barred. |

## Example

    http://localhost:13000/action=AddTask&Type=TelWavToText&File=C:/myData/tel.wav&Out=TelTranscript.ctm&Lang=ENUS

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to perform the `TelWavToText` task on the `tel.wav` file and write the results to the Tel`Transcript.ctm` file. The `tel.wav` file contains U.S. English dialect speech.

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm