Open topic with navigation

# SpeechThresh

The threshold between speech and non-speech (music or noise).

NOTE:

From the 11.2 release, HPE IDOL Speech Server Reference uses a new algorithm for audio preprocessing. The new algorithm uses DNN technology, which provides better performance and requires less tailoring to specific audio types.

The new implementation ignores speech and silence threshold parameters, and also distinguishes between music and noise, rather than simply recognizing music and noise as a single non-speech category. All tasks use the new algorithm, but the old algorithm is retained for backwards compatibility, and can be used in exactly the same way as before.

Action: | AddTask CheckResources
Task: | ClusterSpeech ClusterSpeechTel ClusterSpeechToTextTel LangIdFeature LangIdSegWav LangIdCumWav LangIdBndWav LangIdSegStream LangIdCumStream LangIdBndStream SpeechSilClassification StreamToTextMusicFilter StreamToTextMusicFilterPunct
Type: | Integer
Default: | -25
Range: | -50–10
Example: | `SpeechThresh=0`
See Also: | SpeechThreshOffset (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm