Open topic with navigation

# MinSegSize

The minimum segment size in frames. This value must be lower than MaxSegSize.

NOTE:

Setting `MinSegSize` to a lower value leads to less accuracy. Setting `MinSegSize` to a high value leads to less resolution.

Type: | Integer
Default: | 50
Recommended Range: | Minimum: 20 Maximum: 500
Required: | No
Configuration Section: | audiopreproc module
Example: | `MinSegSize=40`
See Also: | MinSegSize (action parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm