Open topic with navigation

# Image Format Transformation Engine Configuration Parameters

The Image Format transformation engine changes the format of images that are contained in records.

Output engines can output base-64 encoded image data for keyframes, detected or recognized faces, images of number plates, and so on. By default, images produced by HPE Media Server are in PNG format. To output base-64 encoded image data that decodes to another format, use an image format transformation task to modify the image format before sending the data to the output task.

This section describes the parameters that you can use to configure image format transformation.

Configuration Parameter | Description
--- | ---
CompressionQuality | The amount of compression to use for JPEG images.
Format | The image format to convert images into.
Input | The name of the track that contains the data to transform.
Type | The type of transformation engine to use. Set this parameter to `ImageFormat`.

This transformation engine produces a single output track, named `taskName.Output`, where `taskName` is the name of the transformation task.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm