Open topic with navigation

# LabType

The type of labels to use. Set this parameter to `NONE` to switch off labeling. Set this parameter to one of the following options to enable labeling:

- `SID`. Speaker identification output result format.
- `CTM`. Standard output format.
- `LAB`. Label files.

For more information on speaker section labeling, see HPE IDOL Expert.

Action: | AddTask
Task: | IvSpkIdDevel IvSpkIdDevelStream IvSpkIdDevelWav IvSpkIdTrain IvSpkIdTrainStream IvSpkIdTrainWav SpkIdDevel SpkIdDevelStream SpkIdDevelWav SpkIdTrain SpkIdTrainStream SpkIdTrainWav
Type: | String
Default: | `NONE`
Example: | `LabType=SID`
See Also: | LabType (configuration parameter)

© 2015-2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm